**Product Specifications**

Model: VC-X01E, VC-X01D

Wireless Connection: Zigbee

**Dimensions**: 93 × 72 × 84 mm (3.66 × 2.83 × 3.31 in.)

**Battery**: AA Battery × 4

Valve Pressure: 1.6 MPa

Torque: ≤ 3.6 N·m

Valve Opening/Closing Time: 5-20s

**Compatible Pipe Sizes: DN15, DN20, DN25**

**Compatible Handle Types: lever handle, butterfly handle**

Operating temperature: -10°C ~ 50°C (14°C ~ 122°F)

Working Humidity: 0 ~ 95% RH, no condensation

What is in the Box: Valve Controller T1 × 1, User Manual × 1, Accessory Kit × 1, AA Battery × 4

